TRAFFIC INDUSTRIES
Lane channelizers & separators
SPECIFICATION TEXT (draft)
1. Subject and scope
This specification covers the supply of lane channelizers & separators. The function and place of use follow the definition below:
The lane channelizer is a low-profile separator unit fixed to the road to divide two streams physically. A driver can ignore a painted line but feels the lane channelizer through the wheel — where the model profile and the layout allow it, its sloping sides let emergency vehicles cross, and a delineator, cat eye or flap mounts on top. It is low, modular and relocatable. Because its top socket accepts a vertical marker, the lane channelizer becomes one line that warns by contact and by eye. The lane channelizer is used on bus lanes, in cycle-lane separation, at turning pockets, on junction islands and in opposing-flow division.
2. Features
The feature table is given in writing with the quotation.
3. Dimensions and classes
Module length: 1000 mm class — units join end to end
Width: 130–150 mm band
Base height: 50 mm class — sloping sides
Base size (island types): Ø 400 · Ø 450 mm · 300×300 mm
Weight: 0.45–12 kg (by type and top fitting)
Top fitting: Cat eye · flap · post · sign
Total height with top fitting: Follows the chosen post; stated in writing with the quotation
Fixings and parts list: Hole pattern, anchor count and type, included parts (dowels, caps, top-fitting socket) and the removable-mounting option are stated per model on the datasheet; the quotation carries this list
Note: values are production-programme and market-standard ranges; order dimensions are fixed in the quotation.
4. Documentation
Standard names on this page are references; test results and certificates are shared together with the report and the document — ask, and we will send them.
Test results and certificates are shared only with the report and the document; no class name is cited without its document.
5. Packing and delivery
Bodies are palletised stacked · Anchors and fixings travel in separate cartons · Reflective collars ship fitted · Container efficiency is high and volume is the limit
6. Quotation and contact
Quotation requests go through trafficindustries.com; the quotation is prepared the same day against quantity, variant and delivery terms.




