TRAFFIC INDUSTRIES
Traffic barriers
SPECIFICATION TEXT (draft)
1. Subject and scope
This specification covers the supply of traffic barriers. The function and place of use follow the definition below:
The traffic barrier is used to separate a work area or a temporary route from traffic with a visual-physical line. The traffic barrier travels empty and is filled with water or sand on site; its coupling ends join the units into one line. It transports light, sets up fast and redeploys. Its top takes a warning lamp, showing the line at night too. The traffic barrier is used on road works, around site perimeters, at events, and at car park and facility entrances.
2. Features
The feature table is given in writing with the quotation.
3. Dimensions and classes
Body length: 1300–2000 mm (market classes)
Height: 650–1200 mm
Base width: 370–800 mm
Empty weight: 6–41 kg
Water ballast: 60–400 kg
Material: UV-stabilised PE / HDPE
Fill limit and operating weight: The maximum permitted fill volume and the filled operating weight are stated on the model datasheet; the fill mark on the body is not exceeded. In frost conditions the fill choice follows the datasheet instruction
Note: values are production-programme and market-standard ranges; order dimensions are fixed in the quotation.
4. Documentation
Manufactured to the order's specification in the Turkish market. In US language the water-filled traffic barrier is described by the longitudinal channelizing device definition of MUTCD Section 6K.10 (it may be hollow and water-ballasted). These devices are not protection barriers; they are not used to shield obstacles or protect pedestrians or workers. Where impact containment is required, EN 1317-classified systems are a separate conversation. Test results and certificates are shared with the report and the document.
Test results and certificates are shared only with the report and the document; no class name is cited without its document.
5. Packing and delivery
Ships empty — the container is limited by volume, not weight · Bodies nest or stack · Connecting pins travel in separate cartons · Freight cost is markedly lower than for concrete
6. Quotation and contact
Quotation requests go through trafficindustries.com; the quotation is prepared the same day against quantity, variant and delivery terms.




