TRAFFIC INDUSTRIES
Traffic signs
SPECIFICATION TEXT (draft)
1. Subject and scope
This specification covers the supply of traffic signs. The function and place of use follow the definition below:
Traffic signs and folding stands are used to state the rules of a temporary layout to the driver in words and symbols. The reflective face returns headlight to the driver; the folding stand fits the traffic sign and folding stand set into a van, set out by one person. They are portable, fast and readable. The stand takes ballast, staying upright and aligned on a windy site. Traffic signs and folding stands are used on road works, in temporary diversions, in event traffic and in emergency response.
2. Features
The feature table is given in writing with the quotation.
3. Dimensions and classes
Sign / stand size: 49–250 cm
Stand type: Folding tripod · fixed foot · barricade body
Sign face: Reflective sheeting, printed to requirement
Substrate and thickness: Aluminium or galvanised sheet; material, thickness and edge/back stiffening are selected separately per specification — different procurement documents call for different materials and thicknesses, which are not one product’s tolerance band
Delivery scope: Sign face only, or sign + post + clamp package; who is responsible for the foundation and support calculation is fixed in writing before the order
Note: values are production-programme and market-standard ranges; order dimensions are fixed in the quotation.
4. Documentation
Manufactured to the order’s specification in the Turkish market; the governing document is stated in writing at quotation. The reflective class of the sign face is stated in writing per the supplier’s document; class names are cited only with the document. Test results and certificates are shared with the report and the document.
Test results and certificates are shared only with the report and the document; no class name is cited without its document.
5. Packing and delivery
Sign faces and stands are packed separately · Roll-up signs travel in tubes · Spring stands go low on the pallet because of their weight · Print content is set at order
6. Quotation and contact
Quotation requests go through trafficindustries.com; the quotation is prepared the same day against quantity, variant and delivery terms.




